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SECTION 11-14-00
PEDESTRIAN CONTROL EQUIPMENT


PART  1   GENERAL
SECTION INCLUDES
Security Optical Turnstiles of the following type:
Casing, controls, and security system as required for installation. (Speedlane Open Non-Barrier Optical Turnstile)
RELATED SECTIONS
Section 09600- Flooring 
Section 11 14- Pedestrian Control Equipment
Section 11 14 13.19- Turnstiles
Section 11 14.53- Pedestrian Security Equipment
Section 16123- Electrical Supply and Termination
Section 26056- Grounding and Bonding for Electrical Systems
Section 28100- Electronic Access Control and Intrusion Detection
Section 281300- Access Control
Section 281400- Access Control System Hardware
Section 281600- Intrusion Detection
REFERENCES
CSA Group (Canada)
CSA22.2 #247-14, Operators and Systems of Doors, Gates, Draperies and Louvres
Underwriters Laboratories Inc. (UL).
UL Standard 325
UL Standard 2593
SUBMITTALS
Submit under provisions of Section 01 30 00 - Administrative Requirements.
Product Data: Submit manufacturer's product data sheets, including installation details, material descriptions, dimensions of individual components and profiles, fabrication, operational descriptions, and finishes:
Preparation instructions and recommendations.
Storage and handling requirements and recommendations.
Installation methods.
Shop Drawings: Submit manufacturer's shop drawings, including pertinent dimensions, general construction, component connections and locations, anchorage methods and locations, safety plus sensors, hardware, and installation details.
Manufacturer's Project References: Submit list of successfully completed projects including project name and location, name of architect, and type and quantity of turnstiles manufactured.
Manufacturer's Field Reports: Submit manufacturer's field reports from AAADM certified technician of inspection and approval of doors for compliance with ANSI/BHMA 156.27 after completion of installation.
Operation and Maintenance Manual: Submit manufacturer's operation and maintenance manual. 
QUALITY ASSURANCE
Manufacturer's Qualifications:
Specialization in the supply of security optical turnstiles with a minimum of 5 years’ experience.
Factory-Trained supervisor shall be supplied during installation of the security optical turnstile.
Installer's Qualifications:
Local factory-trained field service technician shall be provided to competently service the security turnstile; and to provide for the local support of the customer’s service technicians in the event the customer’s trained technician is not available. In the event there are no service technicians matching the aforementioned description and requirements, the manufacturer, Boon Edam, Inc., is to be utilized for service.
Local certified Boon Edam, Inc. distributor required if not being installed by the manufacturer, Boon Edam, Inc.
Approved by manufacturer.
Single Source Requirements: To the greatest extent possible provide products specified in this section from a single manufacturer.
DELIVERY, STORAGE, AND HANDLING
Delivery: Deliver materials to site protected from damage.
Storage: Store materials in clean, dry area indoors, off ground in manufacturer's unopened packaging until ready for installation and in accordance with manufacturer's instructions.
Handling: Protect materials and finish from damage during handling and installation.
PROJECT CONDITIONS
Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
The Speedlane Open Non-Barrier Optical Turnstile installs on finished floor only.
Floor must be leveled within 5/64” (2 mm) at any point within the footprint of the Speedlane Open array.
Floor must be complete with conduit supplied to meet manufacturer’s specified drawings.
MAINTENANCE SERVICE
The manufacturer shall offer a dispatch procedure that will be available 24 hours per day, 365 days per year to facilitate proper service capability.
A manufacturer's designated service contact shall obtain malfunction information and dispatch appropriate service provider to project location.
Submission for maintenance service via Boon Edam, Inc. Phone: 910-984-8094 or us.techsupport@boonedam.com 
A geographically assigned installation provider shall be trained and certified to provide maintenance service.
COORDINATION AND SCHEDULING
Conference: Convene a pre-installation conference to establish procedures to maintain optimum working conditions and to coordinate this work with related and adjacent work per Owner request.
Coordinate sizes and locations of recesses in concrete if applicable.
Field Measurements: Verify actual dimensions for installation of optical turnstiles by field measurements before fabrication and indicate on shop drawings.
WARRANTY
Warranty: Provide manufacturer's standard warranty against defects in materials and workmanship. Warranty shall be one year from date of installation.
Warranty Period: 1 Year (12 Months) 
During the warranty period a factory-trained technician shall perform service and affect repairs. A safety inspection shall be performed after each adjustment or repair, and a completed inspection form shall be submitted to the Owner.
The Warranty excludes glass breakage, normal wear on finishes or damage that occurs due to abuse, misuse or acts of God.
PART  2   PRODUCTS
MANUFACTURERS
Acceptable Manufacturer: Boon Edam, Inc. 402 McKinney Parkway, Lillington NC 27546. (910) 814-3800 Fax: (910) 814-3889 Website: www.boonedam.us                                    
Substitutions: Not permitted.
Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
SECURITY OPTICAL TURNSTILE
Security Optical Turnstile: Speedlane Open Non- Barrier optical turnstile constructed with stainless steel cabinets as manufactured by Boon Edam, Inc. 
Provide casing manufactured of #4 brushed stainless steel.
Provide Top Plate manufactured from Black Safety Glass
Provide Front Cover Plate manufactured from Black Safety Glass

Finish:
Finishes to be available for the removable panels, bottom of plinth covers, face and top.
Stainless Steel components to be #4 Brushed Satin for the cabinet.
Actuation and Safety Control Devices:
Actuation Devices: Authorization actuation by credential reader mounted under top plate, max dimensions L x W x H: 130mm x 55mm x 50mm (5 7/64” x 2 11/64” x 1 31/32”). (Not supplied by Boon Edam, Inc.)
Actuation: Although a component of the turnstile, actuation devices are provided by the Access Control Integrator.
Controls:
Factory installed, purpose-built microcontroller platform with embedded custom software (Required 110-240 VAC, 1 Phase, 13A service from below).
The Speedlane Open will go into sleep or power saving mode after pre-set time, wake-up detection by sensors in the leading face.
PART  3   EXECUTION
PREPARATION
Installer must examine the location and advise the Contractor of any site conditions unacceptable for proper installation of product. The minimum conditions necessary to initiate installation are:
Floor must be dead level within 5/64” (2mm) at any point within the footprint of the door.
Finished floor must be installed.
Floor must be complete with conduit supplied to meet manufacturer’s specified drawings.
Power supply (110-240VAC) must be installed. Power and communication from floor to the secure side of the cabinet as per approved specified drawings.
INSTALLATION
0. Install turnstile in accordance with manufacturer’s printed instructions. Set unis level, plumb, and with uniform hairline joints. Anchor securely in place. Use only factory trained installers.
FIELD QUALITY CONTROL
Manufacturer's Field Services:
Manufacturer's representative shall provide technical assistance and guidance for installation of Speedlane Open Non-Barrier Optical Turnstile
Before placing optical turnstiles in operation, power supply must be installed. Power and communication come from the floor. Installation shall not begin until these unacceptable conditions are rectified.
ADJUSTING
0. Installer shall adjust turnstile, hardware and sensors for smooth operation and proper performance.
DEMONSTRATION AND TRAINING
0. A factory-trained installer shall demonstrate to the Owner’s maintenance crew the proper operation of the Speedlane Open- Barrier Free Optical Turnstile and the necessary service requirements such as lubrication, cleaning, and inspection of components upon completion of installation.
CLEANING AND PROTECTION
0. Clean metal and glass surfaces carefully using manufacturer’s suggested cleaning materials. 
END OF SECTION
11 14 00 -1 
